[FastNIC]
 Type = NDIS
 Title = "PCI 10/100 Fast Ethernet Adapter"
 Version = 1.00
 DriverName = FSTNIC$
 XPORTS = NETBEUI LANDD

[File]
 Name = FastNIC.OS2
 Path = \NDIS\OS2

[Slot]
 display = "Network Adapter Slot ID."
 type = Decimal
 default = "1"
 range = 1 - 4
 step = 1
 optional = Yes
 editable = Yes
 virtual = No
 help = "This parameter specifies which network adapter is used by the driver.
 If you have only one FastNIC PCI LAN card in your machine, this parameter is
 unnecessary!!  For two or more FastNIC PCI LAN cards, this parameters is
 required and cannot be omitted from PROTOCOL.INI.  The slot ID. for the first
 LAN card is 1, for the second is 2, and 13 for the third, etc.  Default
 value is 1."

[MEDIA]
 display = "Physical Medium Type"
 type = String
 strlength = 14
 default = "AUTODETECT"
 set = AUTODETECT, UTP, UTP_FD, UTP_100,UTP_100FD
 optional = No
 editable = Yes
 virtual = No
 help = "This parameter specifies the physical media that the LAN card is
 attached.  The keyword AUTODETECT means driver will auto sense the physical
 media during card initialization.  TP means twisted-pair (RJ-45 or 10BaseT),
 and UTP_100 means Fast Ethernet.  If you want to enable full duplex function
 of the LAN  card, you have to choose UTP_FD or UTP_100FD as the medium type.
 The default value is AUTODETECT."

