
                 D-Link DFE-530TX PCI Fast Ethernet Adapter

 Contents
 --------

    - Introduction
    - Getting Started
    - Revision History
    - Trouble shooting
    - Support Options
    - Copyrights and Trademarks

 Introduction
 ------------

 To help your friendly installation, you can check it from the
 readme files of INFO directory.  Should there be any further 
 recommendations, please contact with the Local D-Link office listed
 as below.


 Getting Started
 ---------------

    Auto-run program assist your ease of setup.  It will configure
    driver, install appropriate network drivers for popular network
    operating systems on the DFE-530TX adapter.


    You can operate some function through the friendly button:

    1.Install Driver: It will configure driver, install appropriate 
      network drivers for popular network operating systems on the
      DFE-530TX adapter

    2.User's manual: It will show detail manual for your reference.

    3.Go to D-Link Web:You can find other information in our Web and contact 
      with us.
 
    4.Explore CD :It will allow you to explore the CD.

    5.Close Window:You can close Window by this button.
     
    If the NOS (Network Operating System) you are using is not covered
    by the auto-run program, please refer to the individual documentation
    provided in INFO directory.


 Revisions History

    Diskette revision: 20030701
    ---------------------------- 
    -- Support Windows Server 2003. 
    -- Support NetWare 6.5.
    -- Update all drivers.

    Diskette revision: 20030101
    ---------------------------- 
    -- Support 802.1x supplicant.
    -- Support Win Diagnostic,DOS Diagnostic.
    -- Add INFO directory.
    -- Windows 98/ME/2000/XP passed PC99 logo certification.

    Diskette revision: 20020701
    ---------------------------- 
    -- Support DFE-530TX A1/A3/B1/B2/C1 adapters. 

    -- It supports the following drivers:
      --Novell NetWare 3.x, 4.x,5.x,6.x and ODI.DOS.
      --Microsoft Windows NT3.51, NT4.0.
      --Windows 95/95OSR2, 98/98SE/Me,2000/XP.
      --Microsoft Windows for Workgroups 3.11.
      --Microsoft Client for DOS.
      --IBM LAN Support Program v1.3x.
      --FTP PC/TCP.
      --SUN PC-NFS.
      --NDIS 2.x, 3.x, 4.x, 5.x Driver.
      --Packet Driver.
      --Linux Driver. 
    -- Win Diagnostic, SCO OpenServer 5.0, and UnixWare 7.x will be support on
       D-Link Web in the Future. 

    Diskette revision: 20020201
    ---------------------------
    --Add auto-run program.

    Diskette revision: 20011015
    ---------------------------
    -- Update inf file and Windows 98/2000/NT40/ME passed PC99 logo
       certification.

    Diskette revision: 20000615
    ---------------------------
    -- Support DFE-530TX A1/A3/B1 adapters.
    -- Fixed reading of null Mac address when soft-rebooting PC after 
       Windows 98 shutdown.

    Diskette revision: 20000301
    ---------------------------
    -- Flow control function update.
    
    Diskette revision: 20000201
    ---------------------------
    -- Support DFE-530TX A1 and B1
    -- Support WOL, Flow control (DFE-530TX B1 hardware only)

    Diskette revision: 991215
    -------------------------
    -- Support Windows 2000 driver. 
    
    Diskette revision: 990615
    -------------------------
    -- Add NDIS5 drivers for Win98 root file
    -- Win95A/Osr2/Win98 use NDIS3 driver 
       and the same INF file in the root path.

    Diskette revision: 981115
    -------------------------
    --Update NDIS3 and NDIS4 drivers.
    --Update Packet driver.

    Diskette revision: 980915
    -------------------------
    --To update NetWare server driver. 
  
    Diskette revision: 980815
    -------------------------
     --Supports NetWare5.0 driver.
     --To solve "Windows Protection Error" problem.     

    Diskette revision: 980601
    --------------------------
      To solve NEC NX compatible issue under NDIS3 and  NDIS4 drivers.

    Diskette revision: 980515
    -------------------------
      To update Novell NetWare server, NDIS2 and Packet drivers.

    Diskette revision: 980501
    -------------------------
      It supports drivers as the following list.
      --Installation program.
      --Diagnostics program.
      --Novell NetWare 3.12, 4.x, ODI.DOS.
      --Microsoft Windows NT3.51, NT4.0.
      --Windows 95, 98.
      --Microsoft Windows for Workgroups 3.11.
      --IBM LAN Support Program v1.3x.
      --DECnet PathWorks v4.0.
      --Banyan VINES v4.00(2).
      --WIN/TCP PathWay Access for DOS v1.1.
      --FTP PC/TCP.
      --SUN PC-NFS.
      --SCO OpenServer 5.0.
      --NDIS 2.x, 3.x, 4.x Driver.
      --Packet Driver.

    Diskette revision : 980315
    --------------------------
      It supports drivers as the following list.
      --Novell NetWare 3.12, 4.x, ODI.DOS.
      --Microsoft Windows NT3.51, NT4.0.
      --Windows 95, 98.


 Trouble shooting
 ----------------
 During testing of the WOL feature of the DFE-530TX.B1, if you discover  
 the following phenomena:

 1) In WIN98(SE) or WIN2000, if the user turns the Stand By using the normal 
    procedure, then the card can be remote awakened successfully.

 2) If the DFE-530TX.B1 encounters either of the following power-off 
    situations: 
    (a) sudden, abnormal power-down, or (b) PC freezes suddenly, then the WOL
    function fails.
    
    For the second situation, there are two workarounds to re-enable the 
    WOL function:
  
    1. Restart the PC ->
       The PC will scan the harddisk and file system automatically ->
       After the OS is rebooted successfully, turn the Stand By using 
       the normal procedure.

    2. Restart the PC ->
       Enter DOS mode immediately ->
       Use the Setup utility ( please contact with the local D-Link's OBU )
       to re-enable the WOL function.



 Support Options
 ---------------

    For technical support, you may contact your authorized D-Link
    distributor, dealer or the following D-Link branch offices.
    
    D-Link Australia
    Unit 16, 390 Eastern Valley Way 
    Roseville, NSW 2069, 
    Australia
    TEL: 61-2-94177100
    FAX: 61-2-94171077
    URL: www.dlink.com.au



    D-Link Canada
    #2180 Winston Park Drive 
    Oakville, Ontario, L6H 5W1
    Canada
    TEL: 1-905-8295033
    FAX: 1-905-8295095
    URL: www.dlink.ca



    D-Link South America
    Isidora Goyeechea 2934 of 702,
    Las Condes
    Santiago ¡V Chile S.A.
    TEL: 56-2-232-3185
    FAX: 56-2-232-0923
    URL: www.dlink.cl



    D-Link Denmark
    Naverland 2, DK-2600
    Glostrup, Copenhagen,
    Denmark
    TEL: 45-43-969040
    FAX: 45-43-424347
    URL:www.dlink.dk



    D-Link Middle East
    7 Assem Ebn Sabet Street Heliopolis Cairo 
    Egypt
    TEL: 202-2456176
    FAX: 202-2456192
    URL: www.dlink-me.com




    D-Link France
    Le Florilege #.2, Allee de la Fresnerie 
    78330 Fontenay le Fleury 
    France
    TEL: 33-1-30238688
    FAX: 33-1-30238689
    URL: www.dlink-france.fr



    D-Link Germany
    Schwalbacher Stra_e 74
    65760 Eschborn
    Germany
    TEL: 49-6196-77990
    FAX: 49-6196-7799300
    URL: www.dlink.de



    D-Link India
    Plot No.5, Kurla-Bandra Complex Rd. 
    Off Cst Rd. Santacruz (E), Bombay - 400 098
    India
    TEL: 91-22-652-6696
    FAX: 91-22-652-8914
    URL: www.dlink-india.com




    D-Link Italia
    via Nino Bonnet n. 6/b
    20154 ¡V Milano,
    Italy
    TEL: 39-02-2900-0676
    FAX: 39-02-2900-1723
    URL: www.dlink.it



    D-Link Japan
    10F, 8-8-15 Nishi-Gotanda 
    Shinagawa-ku, Tokyo 141, 
    Japan
    TEL: 81-3-5434-9678
    FAX: 81-3-5434-9868
    URL: www.d-link.co.jp 




    D-Link Russia 
    Michurinski Prospekt 49, 
    117607 Moscow, 
    Russia
    TEL: 7-095-737-3389, 7-095-737-3492
    FAX: 7-095-737-3390




    D-Link International (Singapore)
    1 International Bussiness Park
    #03-12 The Synergy 
    Singapore 609917
    TEL: 65-774-6233
    FAX: 65-774-6322
    URL: www.dlink-intl.com   



    D-Link South Africa
    Unit 2, Parkside 86 Oak Avenue
    Highveld Technopark Centurion 
    Gauteng 
    Republic of South Africa
    TEL: 27(0)126652165
    FAX: 27(0)126652186




    D-Link Sweden
    P.O. Box 15036, S-167 15 Bromma
    Sweden
    TEL: 46-(0)8564-61900
    FAX: 46-(0)8564-61901
    URL: www.dlink.se



    D-Link Taiwan
    2F, No. 119 Pao-Chung Rd. 
    Hsin-Tien, Taipei 
    Taiwan
    TEL: 886-2-2910-2626
    FAX: 886-2-2910-1515
    URL: www.dlinktw.com.tw



    D-Link U.K.(Europe)
    4th Floor, Merit House
    Edgware Road, Colindale
    London NW9 5AB
    U.K.
    TEL: 44-20-8731-5555
    FAX: 44-20-8731-5511
    BBS: 44-181-235-5511
    URL: www.dlink.co.uk




    D-Link U.S.A
    53 Discovery Drive 
    Irvine, CA 92618
    U.S.A.
    TEL: 1-949-788-0805
    FAX: 1-949-753-7033
    URL: www.dlink.com

                      
 
    The BBS communication setup information is as follows :

    Speed     :  2400-14400  baud                           - Germany
                 2400-9600   baud                           - Asia,Taiwan
                 14400-16800 baud                           - Canada
                 9600-14400  baud V32, V32bis, V42, V42bis  - U.S.A.
                 2400-19200  baud V24, V32, V32bis, V42bis  - U.K. & Europe
    Parity    : none
    Data bits : 8
    Stop bit  : 1

 Copyrights, Trademarks
 ======================
    All documents and software provided herewith are Copyright (c)2002
    D-Link Corporation. All rights reserved.

    Windows 95/95OSR2, 98/98SE/Me,2000/XP/Server 2003, NT 4.0 are trade 
    names of Microsoft Corporation.

    Other trademarks or trade names used herein are properties of the
    respective owners.

