[DCNND2]
 Type = NDIS
 Title = "DigitalChina DCN-530TX Fast Ethernet Adapter."
 Version = 1.00
 DriverName = DCNND2$
 XPORTS = NETBEUI LANDD

[File]
 Name = DCNND2.DOS
 
[Slot]
 display = "Network Adapter Slot ID."
 type = Decimal
 default = "1"
 range = 1 - 4
 step = 1
 optional = Yes
 editable = Yes
 virtual = No
 help = "This parameter specifies which network adapter is used by the driver.
 If you have only one DigitalChina DCN-530TX Fast Ethernet Adapter in your machine
 , this parameter is unnecessary!! For two or more DigitalChina DCN-530TX Fast 
 Ethernet Adapter, this parameters is required and cannot be omitted from PROTOCOL
 .INI. The slot ID. for the first LAN card is 1, for the second is 2, and 3 for the
 third, etc.  Default value is 1."

[MEDIA]
 display = "Physical Medium Type"
 type = String
 strlength = 14
 default = "AUTODETECT"
 set = AUTODETECT, UTP, UTP_FD, UTP_100,UTP_100FD
 optional = No
 editable = Yes
 virtual = No
 help = "This parameter specifies the physical media that the LAN card is
 attached.  The keyword AUTODETECT means driver will auto sense the physical
 media during card initialization. UTP means twisted-pair (RJ-45 or 10BaseT),
 and UTP_100 means Fast Ethernet. If you want to enable full duplex function
 of the LAN  card, you have to choose UTP_FD or UTP_100FD as the medium type.
 The default value is AUTODETECT."

