;DrIvEr DeScRiPtIoN
;
;       Novell NetWare Server Driver Description File for FastNIC.LAN
;

VER: 1.12
SYN: 1.00

DR FastNIC
{
	DES:    "PCI 10/100 Fast Ethernet Adapter (32-Bit ODI)"
	HELP:   "This driver supports PCI bus type."
	PAR:    2.00
	PROD:   'PCI.1317.0981.1113.1216.*',
		'PCI.1317.0985.*.*.*',
		'PCI.1317.1985.*.*.*',
		'PCI.1011.0019.*.*.*',
		'PCI.1011.0009.*.*.*',
		'PCI.1317.9511.1317.9511.*',
		'PCI.1317.9513.1317.9513.*'

		

	FILE:   FastNIC.LAN
	TIME:   15

	PR SLOT REQ
	{
	  VAL: 1-65535
	}

	FRAME Frame_Type
	{
		CD:  'Ethernet_802.2'
		CH:  'Ethernet_802.2'
		CD:  'Ethernet_802.3'
		CH:  'Ethernet_802.3'
		CD:  'Ethernet_SNAP'
		CH:  'Ethernet_SNAP'
		CD:  'Ethernet_II'
		CH:  'Ethernet_II'
		DEF:    1,2,3,4
	}

	LIST Media_Type OPTIONAL
	{
		DES:    $FastNIC_1
		HELP:   $FastNIC_2
		CD:     $FastNIC_3
		CH:     $FastNIC_4
		CD:     $FastNIC_5
		CH:     $FastNIC_6
		CD:     $FastNIC_7
		CH:     $FastNIC_8
		CD:     $FastNIC_9
		CH:     $FastNIC_10
		CD:     $FastNIC_11
		CH:     $FastNIC_12
		DEF:    UNDEFINED
		OUT:    '%s'
	}
	PROMPT TXTHRESHOLD OPTIONAL
	{
		DES:                          $FastNIC_13
		HELP:                         $FastNIC_14
		TYPE:                         DECIMAL
		Value:                        0 - 4
		DEF:                          UNDEFINED
		OUTPUTFORMAT:                 'TXTHRESHOLD=%s'
	}

	PROMPT NODE
	{
	}
}

DLANG:  4
;English
	$FastNIC_1    = "Connection Media Type"
	$FastNIC_2    = "Please choose the media type that you would like to use."
	$FastNIC_3    = "Auto Detection Media"
	$FastNIC_4    = "AUTO"
	$FastNIC_5    = "10 BaseT"
	$FastNIC_6    = "10-HD"
	$FastNIC_7    = "10 BaseT Full-Duplex"
	$FastNIC_8    = "10-FD"
	$FastNIC_9    = "100 BaseTx"
	$FastNIC_10   = "100-HD"
	$FastNIC_11   = "100 BaseTx Full-Duplex"
	$FastNIC_12   = "100-FD"
	$FastNIC_13   = "Tx Threshold"
	$FastNIC_14   = "Tx Threshold can be set 0~3, 4 is Store forward"
	$FastNIC_15   = "0"
	$FastNIC_19   = "4"

LANG:   6
;French
	$FastNIC_1    = "Connection Media Type"
	$FastNIC_2    = "Please choose the media type that you would like to use."
	$FastNIC_3    = "Auto Detection Media"
	$FastNIC_4    = "AUTO"
	$FastNIC_5    = "10 BaseT"
	$FastNIC_6    = "10-HD"
	$FastNIC_7    = "10 BaseT Full-Duplex"
	$FastNIC_8    = "10-FD"
	$FastNIC_9    = "100 BaseTx"
	$FastNIC_10   = "100-HD"
	$FastNIC_11   = "100 BaseTx Full-Duplex"
	$FastNIC_12   = "100-FD"
	$FastNIC_13   = "Tx Threshold"
	$FastNIC_14   = "Tx Threshold can be set 0~3, 4 is Store forward"
	$FastNIC_15   = "0"
	$FastNIC_19   = "4"

LANG:   7
;German
	$FastNIC_1    = "Connection Media Type"
	$FastNIC_2    = "Please choose the media type that you would like to use."
	$FastNIC_3    = "Auto Detection Media"
	$FastNIC_4    = "AUTO"
	$FastNIC_5    = "10 BaseT"
	$FastNIC_6    = "10-HD"
	$FastNIC_7    = "10 BaseT Full-Duplex"
	$FastNIC_8    = "10-FD"
	$FastNIC_9    = "100 BaseTx"
	$FastNIC_10   = "100-HD"
	$FastNIC_11   = "100 BaseTx Full-Duplex"
	$FastNIC_12   = "100-FD"
	$FastNIC_13   = "Tx Threshold"
	$FastNIC_14   = "Tx Threshold can be set 0~3, 4 is Store forward"
	$FastNIC_15   = "0"
	$FastNIC_19   = "4"


LANG:   8
;Italian
	$FastNIC_1    = "Connection Media Type"
	$FastNIC_2    = "Please choose the media type that you would like to use."
	$FastNIC_3    = "Auto Detection Media"
	$FastNIC_4    = "AUTO"
	$FastNIC_5    = "10 BaseT"
	$FastNIC_6    = "10-HD"
	$FastNIC_7    = "10 BaseT Full-Duplex"
	$FastNIC_8    = "10-FD"
	$FastNIC_9    = "100 BaseTx"
	$FastNIC_10   = "100-HD"
	$FastNIC_11   = "100 BaseTx Full-Duplex"
	$FastNIC_12   = "100-FD"
	$FastNIC_13   = "Tx Threshold"
	$FastNIC_14   = "Tx Threshold can be set 0~3, 4 is Store forward"
	$FastNIC_15   = "0"
	$FastNIC_19   = "4"

LANG:   14
;Spanish
	$FastNIC_1    = "Connection Media Type"
	$FastNIC_2    = "Please choose the media type that you would like to use."
	$FastNIC_3    = "Auto Detection Media"
	$FastNIC_4    = "AUTO"
	$FastNIC_5    = "10 BaseT"
	$FastNIC_6    = "10-HD"
	$FastNIC_7    = "10 BaseT Full-Duplex"
	$FastNIC_8    = "10-FD"
	$FastNIC_9    = "100 BaseTx"
	$FastNIC_10   = "100-HD"
	$FastNIC_11   = "100 BaseTx Full-Duplex"
	$FastNIC_12   = "100-FD"
	$FastNIC_13   = "Tx Threshold"
	$FastNIC_14   = "Tx Threshold can be set 0~3, 4 is Store forward"
	$FastNIC_15   = "0"
	$FastNIC_19   = "4"

;DrIvEr DeScRiPtIoN EnD

