;**************************************************************************
;             Copyright 2001-2002 ADMtek Incorporated.
;          Windows 2000 & Win98 combined inf for NDIS5 driver
;**************************************************************************

[version]
Signature   = "$CHICAGO$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ADMtek%
;LayoutFile  = layout.inf                             ;; for put-on-list
CatalogFile = netadm9x.cat                            ;; for WHQL certified
DriverVer   = 10/25/2001, 2.17.1025.2001

[Manufacturer]
%ADMtek% = ADMtek

[ControlFlags]
ExcludeFromSelect = \
			PCI\VEN_1317&DEV_0985, \
			PCI\VEN_1317&DEV_0985&SUBSYS_12161113, \
			PCI\VEN_1317&DEV_0985&SUBSYS_3181109F, \
			PCI\VEN_1317&DEV_0985&SUBSYS_95101317, \
			PCI\VEN_1317&DEV_1985, \
			PCI\VEN_1317&DEV_1985&SUBSYS_12161113, \
			PCI\VEN_1317&DEV_9511, \
			PCI\VEN_1317&DEV_9511&SUBSYS_01131054, \
			PCI\VEN_1317&DEV_9511&SUBSYS_2002155D, \
			PCI\VEN_1317&DEV_9511&SUBSYS_400D144F, \
			PCI\VEN_1317&DEV_9511&SUBSYS_95111317, \
			PCI\VEN_1317&DEV_9513, \
			PCI\VEN_1317&DEV_9513&SUBSYS_95131317, \
			PCI\VEN_1113&DEV_1216&SUBSYS_22421113

[ADMtek]
%AN983Based.DeviceDesc%   = AN983Based.ndi,     PCI\VEN_1317&DEV_0985
%AN983.DeviceDesc%        = AN983.ndi,          PCI\VEN_1317&DEV_0985&SUBSYS_12161113
%AN983.DeviceDesc%        = AN983TG.ndi,        PCI\VEN_1317&DEV_0985&SUBSYS_3181109F
%AN985Based.DeviceDesc%   = AN985Based.ndi,     PCI\VEN_1317&DEV_1985
%AN985.DeviceDesc%        = AN985.ndi,          PCI\VEN_1317&DEV_1985&SUBSYS_12161113
%ADM9510.DeviceDesc%      = ADM9510.ndi,        PCI\VEN_1317&DEV_0985&SUBSYS_95101317
%ADM9511Based.DeviceDesc% = ADM9511Based.ndi,   PCI\VEN_1317&DEV_9511
%ADM9511.DeviceDesc%      = ADM9511.ndi,        PCI\VEN_1317&DEV_9511&SUBSYS_95111317
%ADM9511.DeviceDesc%      = ADM9511NEC.ndi,     PCI\VEN_1317&DEV_9511&SUBSYS_400D144F
%ADM9511.DeviceDesc%      = ADM9511HITACHI.ndi, PCI\VEN_1317&DEV_9511&SUBSYS_01131054
%ADM9511.DeviceDesc%      = ADM9511TG.ndi,      PCI\VEN_1317&DEV_9511&SUBSYS_2002155D
%ADM9513Based.DeviceDesc% = ADM9513Based.ndi,   PCI\VEN_1317&DEV_9513
%ADM9513.DeviceDesc%      = ADM9513.ndi,        PCI\VEN_1317&DEV_9513&SUBSYS_95131317
%AN983.DeviceDesc%        = EN2242.ndi,         PCI\VEN_1113&DEV_1216&SUBSYS_22421113

;----------------------------
; Windows 98                 
;----------------------------
[AN983Based.ndi]
AddReg          = AN983Based.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[AN983.ndi]
AddReg          = AN983.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[AN983TG.ndi]
AddReg          = AN983TG.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles


[AN985Based.ndi]
AddReg          = AN985Based.Reg, ADM9X.common.Reg, ADM9X.cardbus.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[AN985.ndi]
AddReg          = AN985.Reg, ADM9X.common.Reg, ADM9X.cardbus.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[ADM9510.ndi]
AddReg          = ADM9510.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[ADM9511Based.ndi]
AddReg          = ADM9511Based.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[ADM9511.ndi]
AddReg          = ADM9511.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[ADM9511NEC.ndi]
AddReg          = ADM9511NEC.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[ADM9511HITACHI.ndi]
AddReg          = ADM9511HITACHI.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[ADM9511TG.ndi]
AddReg          = ADM9511TG.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[ADM9513Based.ndi]
AddReg          = ADM9513Based.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[ADM9513.ndi]
AddReg          = ADM9513.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

[EN2242.ndi]
AddReg          = EN2242.Reg, ADM9X.common.Reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles

;----------------------------
; Windows 2000               
;----------------------------
[AN983Based.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = AN983.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[AN983Based.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[AN983.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = AN983.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[AN983.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[AN983TG.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = AN983.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[AN983TG.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9510.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = AN983.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[ADM9510.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[AN985Based.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = AN985.ndi.reg, ADM9X.ndi.common.reg, ADM9X.cardbus.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[AN985Based.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[AN985.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = AN985.ndi.reg, ADM9X.ndi.common.reg, ADM9X.cardbus.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[AN985.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9511Based.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = ADM9511.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[ADM9511Based.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9511.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = ADM9511.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[ADM9511.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9511NEC.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = ADM9511.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[ADM9511NEC.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9511HITACHI.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = ADM9511.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[ADM9511HITACHI.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9511TG.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = ADM9511.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[ADM9511TG.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9513Based.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = ADM9513.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[ADM9513Based.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9513.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = ADM9513.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[ADM9513.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[EN2242.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = EN2242.ndi.reg, ADM9X.ndi.common.reg, ADM9X.pci.reg, ADM9X.con.reg
CopyFiles       = ADM9X.ndis.copyfiles.NT

[EN2242.ndi.NT.Services]
AddService      = ADM9X, 2, ADM9X.Service, ADM9X.EventLog


[ADM9X.ndis.copyfiles]
ADM9X.sys,,,2

[ADM9X.ndis.copyfiles.NT]
ADM9X.sys,,,2


;-------------------------------------------------------------------------
; Windows 98 Parameters
;-------------------------------------------------------------------------
;; key,subkey,valuname,type,value
[AN983Based.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_0985"
HKR,               , AdapterCFID,       , 09851317

[AN983.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_0985&SUBSYS_12161113"
HKR,               , AdapterCFID,       , 09851317

[AN983TG.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_0985&SUBSYS_3181109F"
HKR,               , AdapterCFID,       , 09851317

[AN985Based.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_1985"
HKR,               , AdapterCFID,       , 19851317

[AN985.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_1985&SUBSYS_12161113"
HKR,               , AdapterCFID,       , 19851317

[ADM9510.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_0985&SUBSYS_95101317"
HKR,               , AdapterCFID,       , 09851317

[ADM9511Based.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_9511"
HKR,               , AdapterCFID,       , 95111317

[ADM9511.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_9511&SUBSYS_95111317"
HKR,               , AdapterCFID,       , 95111317

[ADM9511NEC.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_9511&SUBSYS_400D144F"
HKR,               , AdapterCFID,       , 95111317

[ADM9511HITACHI.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_9511&SUBSYS_01131054"
HKR,               , AdapterCFID,       , 95111317

[ADM9511TG.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_9511&SUBSYS_2002155D"
HKR,               , AdapterCFID,       , 95111317

[ADM9513Based.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_9513"
HKR,               , AdapterCFID,       , 95131317

[ADM9513.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1317&DEV_9513&SUBSYS_95131317"
HKR,               , AdapterCFID,       , 95131317

[EN2242.Reg]
HKR, NDI,            DeviceID,          , "PCI\VEN_1113&DEV_1216&SUBSYS_22421113"
HKR,               , AdapterCFID,       , 12161113



[ADM9X.common.Reg]
HKR,               , DevLoader,         , *ndis
HKR,               , DeviceVxDs,        , ADM9X.sys

;;Parameters
HKR,               , AdapterType,       , 5
HKR,               , BusType,           , 5

;;NDIS Info
HKR, NDIS,           MajorNdisVersion, 1, 04
HKR, NDIS,           MinorNdisVersion, 1, 00
HKR, NDIS,           LogDriverName,     , "ADM9X"

;;Interfaces
HKR, Ndi\Interfaces, DefUpper,          , "ndis3"
HKR, Ndi\Interfaces, DefLower,          , "ethernet"
HKR, Ndi\Interfaces, UpperRange,        , "ndis3"
HKR, Ndi\Interfaces, LowerRange,        , "ethernet"

;;Install sections
HKR, Ndi\Install,    ndis3,            0, "ADMtek.Install"


;-------------------------------------------------------------------------
; Windows 2000 Parameters
;-------------------------------------------------------------------------
[AN983.ndi.reg]
HKR,               , AdapterCFID,      0, "09851317"

[AN985.ndi.reg]
HKR,               , AdapterCFID,      0, "19851317"

[ADM9511.ndi.reg]
HKR,               , AdapterCFID,      0, "95111317"

[ADM9513.ndi.reg]
HKR,               , AdapterCFID,      0, "95131317"

[EN2242.ndi.reg]
HKR,               , AdapterCFID,      0, "12161113"

[ADM9X.ndi.common.reg]
HKR, Ndi,            Service,          0, "ADM9X"
HKR, Ndi\Interfaces, LowerRange,       0, "ethernet"
HKR, Ndi\Interfaces, UpperRange,       0, "ndis5"
HKR,               , MediaType,        0, "0"

;-------------------------------------------------------------------------
; ADM9X PCI Parameters
;-------------------------------------------------------------------------
[ADM9X.pci.reg]
HKR, , AdapterType,    0, "5"
HKR, , PacketsPerTxInt, , "10"       ; 0x0a
HKR, , PacketsPerRxInd, , "10"       ; 0x0a
HKR, , BurstLength,     , "0"        ; 0(Unlimited), 1 DW, 2 DW, 3 DW,...
HKR, , TxPacketDesc,    , "300"
HKR, , RxPacketDesc,    , "120"      ; 0x78
HKR, , TxDmaDesc,       , "600"
HKR, , RxDmaDesc,       , "40"       ; 0x28

[ADM9X.cardbus.reg]
HKR, , AdapterType,    0, "5"
HKR, , PacketsPerTxInt, , "10"       ; 0x0a
HKR, , PacketsPerRxInd, , "10"       ; 0x0a
HKR, , BurstLength,     , "0"        ; 0(Unlimited), 1 DW, 2 DW, 3 DW,...
HKR, , TxPacketDesc,    , "300"
HKR, , RxPacketDesc,    , "120"      ; 0x78
HKR, , TxDmaDesc,       , "900"
HKR, , RxDmaDesc,       , "40"       ; 0x28


;-------------------------------------------------------------------------
; ADM9X Common Parameters
;-------------------------------------------------------------------------
[ADM9X.con.reg]
HKR, Ndi\Params\MediaType,            ParamDesc,  , "Media Type"
HKR, Ndi\Params\MediaType,            default,    , "0"
HKR, Ndi\Params\MediaType,            type,       , "enum"
HKR, Ndi\Params\MediaType\enum,       0,          , "AutoSense"
HKR, Ndi\Params\MediaType\enum,       1,          , "10BaseT"
HKR, Ndi\Params\MediaType\enum,       2,          , "10BaseT Full_Duplex"
HKR, Ndi\Params\MediaType\enum,       3,          , "100BaseTX"
HKR, Ndi\Params\MediaType\enum,       4,          , "100BaseTX Full_Duplex"
HKR, Ndi\Params\MediaType,            flag,      1, "20","00","00","00"

HKR, Ndi\Params\PowerManagement,      ParamDesc,  , "PME Enable"
HKR, Ndi\Params\PowerManagement,      default,    , "1"
HKR, Ndi\Params\PowerManagement,      type,       , "enum"
HKR, Ndi\Params\PowerManagement\enum, 0,          , "Disabled"
HKR, Ndi\Params\PowerManagement\enum, 1,          , "Enabled"
HKR, Ndi\Params\PowerManagement,      flag,      1, "20","00","00","00"

HKR, Ndi\Params\WakeupFrame,          ParamDesc,  , "Pattern Match Wakeup"
HKR, Ndi\Params\WakeupFrame,          default,    , "1"
HKR, Ndi\Params\WakeupFrame,          type,       , "enum"
HKR, Ndi\Params\WakeupFrame\enum,     0,          , "Disabled"
HKR, Ndi\Params\WakeupFrame\enum,     1,          , "Enabled"
HKR, Ndi\Params\WakeupFrame,          flag,      1, "20","00","00","00"

HKR, Ndi\Params\LinkOnChange,         ParamDesc,  , "Link Wakeup(Off->On)"
HKR, Ndi\Params\LinkOnChange,         default,    , "1"
HKR, Ndi\Params\LinkOnChange,         type,       , "enum"
HKR, Ndi\Params\LinkOnChange\enum,    0,          , "Disabled"
HKR, Ndi\Params\LinkOnChange\enum,    1,          , "Enabled"
HKR, Ndi\Params\LinkOnChange,         flag,      1, "20","00","00","00"
 
HKR, Ndi\Params\LinkOffChange,        ParamDesc,  , "Link Wakeup(On->Off)"
HKR, Ndi\Params\LinkOffChange,        default,    , "0"
HKR, Ndi\Params\LinkOffChange,        type,       , "enum"
HKR, Ndi\Params\LinkOffChange\enum,   0,          , "Disabled"
HKR, Ndi\Params\LinkOffChange\enum,   1,          , "Enabled"
HKR, Ndi\Params\LinkOffChange,        flag,      1, "20","00","00","00"

HKR, Ndi\Params\MagicPacket,          ParamDesc,  , "Magic Packet Wakeup"
HKR, Ndi\Params\MagicPacket,          default,    , "1"
HKR, Ndi\Params\MagicPacket,          type,       , "enum"
HKR, Ndi\Params\MagicPacket\enum,     0,          , "Disabled"
HKR, Ndi\Params\MagicPacket\enum,     1,          , "Enabled"
HKR, Ndi\Params\MagicPacket,          flag,      1, "20","00","00","00"

HKR, Ndi\Params\FlowControl,          ParamDesc,  , "Flow Control"
HKR, Ndi\Params\FlowControl,          default,    , "1"
HKR, Ndi\Params\FlowControl,          type,       , "enum"
HKR, Ndi\Params\FlowControl\enum,     0,          , "Disabled"
HKR, Ndi\Params\FlowControl\enum,     1,          , "Enabled"
HKR, Ndi\Params\FlowControl,          flag,      1, "20","00","00","00"

HKR, Ndi\Params\PriorityPacket,       ParamDesc,  , "Priority Packet"
HKR, Ndi\Params\PriorityPacket,       default,    , "0"
HKR, Ndi\Params\PriorityPacket,       type,       , "enum"
HKR, Ndi\Params\PriorityPacket\enum,  0,          , "Disabled"
HKR, Ndi\Params\PriorityPacket\enum,  1,          , "Enabled"
HKR, Ndi\Params\PriorityPacket,       flag,      1, "20","00","00","00"

HKR,Ndi\params\VlanId,                ParamDesc, 0, "VLAN ID"
HKR,Ndi\params\VlanId,                type,      0, "edit"
HKR,Ndi\params\VlanId,                default,   0, "0"
HKR,Ndi\params\VlanId,                LimitText, 0, "4"
HKR,Ndi\params\VlanId,                UpperCase, 0, "1"
HKR,Ndi\params\VlanId,                Optional,  0, "1"

;-------------------------------------------------------------------------
; Service
;-------------------------------------------------------------------------
[ADM9X.Service]
DisplayName     = %ADM9X.Service.DispName%
ServiceType     = 1                                ;%SERVICE_KERNEL_DRIVER%
StartType       = 3                                ;%SERVICE_AUTO_START%
ErrorControl    = 1                                ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\ADM9X.sys
LoadOrderGroup  = NDIS
AddReg          = TextModeFlags.reg

[ADM9X.EventLog]
AddReg = ADM9X.AddEventLog.reg

[ADM9X.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR, , TypesSupported,   0x00010001, 7

[TextModeFlags.reg]
HKR, , TextModeFlags, 0x00010001, 0x0001


;-------------------------------------------------------------------------
; Destination Directory
;-------------------------------------------------------------------------
[DestinationDirs]
ADM9X.ndis.copyfiles     = 11
ADM9X.ndis.copyfiles.NT  = 12
DefaultDestDir           = 11                  ; LDID_SYS


;-------------------------------------------------------------------------
; Source Files
;-------------------------------------------------------------------------
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
ADM9X.sys = 1
netadm9x.inf = 1
netadm9x.cat = 1


;-------------------------------------------------------------------------
; Strings
;-------------------------------------------------------------------------
[Strings]
;;Msft    = "Microsoft"
ADMtek  ="ADMtek Incorporated."

;;Source Disk Name
DISKNAME = "ADMtek AN983/AN985/ADM951X 10/100Mbps Fast Ethernet Adapter Driver Diskette "

AN983Based.DeviceDesc   = "ADMtek AN983 Based Fast Ethernet Adapter"
AN985Based.DeviceDesc   = "ADMtek AN985 Based Fast Ethernet Adapter"
ADM9511Based.DeviceDesc = "ADMtek ADM9511 Based Fast Ethernet Adapter"
ADM9513Based.DeviceDesc = "ADMtek ADM9513 Based Fast Ethernet Adapter"
AN983.DeviceDesc        = "ADMtek AN983 10/100Mbps Fast Ethernet Adapter"
AN985.DeviceDesc        = "ADMtek AN985 10/100Mbps Fast Ethernet Adapter"
ADM9510.DeviceDesc      = "ADMtek ADM9510 10/100Mbps Fast Ethernet Adapter"
ADM9511.DeviceDesc      = "ADMtek ADM9511 10/100Mbps Fast Ethernet Adapter"
ADM9513.DeviceDesc      = "ADMtek ADM9513 10/100Mbps Fast Ethernet Adapter"
ADM9X.Service.DispName  = "ADMtek AN983/AN985/ADM951X 10/100Mbps Fast Ethernet Adapter"

